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논문·기술 자료 요약 — 오늘 쓸 재료
아래 글을 그대로 복사해 Claude 채팅 창의 부탁 문장 아래에 붙여 넣으세요.
[자료] Effect of Shot Peening Intensity on the Fatigue Life of
       A356 Aluminum Suspension Brackets (가상 자료, 4쪽 PDF)
[핵심 문장 일부]
 - Brackets were shot peened at 0.15, 0.25 and 0.35 mmA ... (p.2)
 - Peening at 0.25 mmA increased mean fatigue life by 2.1 times ... (p.3, Table 2)
 - At 0.35 mmA, surface roughness rose to Ra 3.2 µm ... (p.3)
 - Only six specimens per condition were tested. No corrosion testing was performed. (p.4)
[우리 상황]
 - 대현테크 연구소, 알루미늄 서스펜션 브래킷 시제품 개발 중
 - 숏피닝 설비는 사내에 없음, 외주 가능 여부 (확인 필요)
 - 고객 요구: 피로 수명 향상 + 염수 환경 내구성




